

**Cisco 2800 VPN related configuration**

**crypto isakmp policy 15**

**encryption 3des**

**hash md5**

**authentication pre-share**

**group 2**

**lifetime 28800**

**!**

**crypto isakmp key golfTDI130 address 83.206.43.38**

**!**

**crypto ipsec transform-set vpn esp-3des esp-md5-hmac**

**!**

**crypto map vpn 1 ipsec-isakmp**

**set peer 83.206.43.38**

**set transform-set vpn**

**set pfs group2**

[**match**](http://www.techcity.cgngroup.com/tag/ipsec-vpn-between-juniper-netscreen-ssg-5-and-cisco-ios-router/) **address 101**

**!**

**interface Ethernet0**

**description Inside Interface**

**ip address 172.16.0.254 255.255.255.0**

**!**

**interface Ethernet1**

**description Outside Interface**

**ip address 192.168.200.2 255.255.255.0**

**crypto map vpn**

**!**

**ip route 0.0.0.0 0.0.0.0 192.168.200.1**

**!**

**access-list 101  permit ip 172.16.0.0 0.0.0.255 192.168.0.0 0.0.1.255**

**permit ip 192.168.1.0 0.0.0.255 192.168.55.0 0.0.0.255**