# Site A firewall Configuration

Disabled Interface monitor for Ethernet3/0 under NSRP interface monitoring



Enabled Track IP under ethernet3/0 interface>Monitor



**Routes for Site B**

set route 192.168.88.0/21 interface ethernet3/0 gateway 17.10.10.5

set route 10.135.80.0/24 interface ethernet3/0 gateway 17.10.10.5

set route 10.0.84.0/22 interface ethernet3/0 gateway 17.10.10.5

**Backup Routes for Site B**

set route 192.168.88.0/21 interface tunnel.24 metric 2

set route 10.0.84.0/22 interface tunnel.24 metric 2

set route 10.135.80.0/24 interface tunnel.24 metric 2

**Interface Configuration**

set interface "ethernet3/0" zone "Trust"

set interface ethernet3/0 ip 17.10.10.6/29

set interface ethernet3/0 nat

set interface ethernet3/0 manage-ip 17.10.10.4

set interface ethernet3/0 monitor track-ip ip

set interface ethernet3/0 monitor track-ip ip 17.10.10.5 interval 2

unset interface ethernet3/0 monitor track-ip dynamic

# Site B firewalls configuration

Disabled Ethernet3/0 interface monitor under NSRP



Enabled Track IP under ethernet3/0 interface>Monitor





## Static Routes for Site A

set route 192.168.160.0/21 interface ethernet3/0 gateway 17.10.10.6

set route 192.168.159.0/24 interface ethernet3/0 gateway 17.10.10.6

set route 192.168.116.0/24 interface ethernet3/0 gateway 17.10.10.6

## Backup Routes for Site A

set route 192.168.160.0/21 interface tunnel.20 metric 2 description "Backup route for P2P link"

set route 192.168.48.0/21 interface tunnel.20 metric 2

set route 192.168.159.0/24 interface tunnel.20 metric 2

**Interface Configuration**

set interface "ethernet3/0" zone "Trust"

set interface ethernet3/0 ip 17.10.10.5/29

set interface ethernet3/0 nat

set interface ethernet3/0 monitor track-ip ip

set interface ethernet3/0 monitor track-ip threshold 2

set interface ethernet3/0 monitor track-ip ip 17.10.10.6 interval 2

unset interface ethernet3/0 monitor track-ip dynamic