SSG_FW1-> get config
Total Config size 4024:
set clock timezone 0
set vrouter trust-vr sharable
set vrouter "untrust-vr"
exit
set vrouter "trust-vr"
unset auto-route-export
exit
set auth-server "Local" id 0
set auth-server "Local" server-name "Local"
set auth default auth server "Local"
set auth radius accounting port 1646
set admin name "netscreen"
set admin password "nKVUM2rwMUzPcrkG5sWIHdCtqkAibn"
set admin auth timeout 10
set admin auth server "Local"
set admin format dos
set zone "Trust" vrouter "trust-vr"
set zone "Untrust" vrouter "trust-vr"
set zone "DMZ" vrouter "trust-vr"
set zone "VLAN" vrouter "trust-vr"
set zone "Untrust-Tun" vrouter "trust-vr"
set zone "Trust" tcp-rst 
set zone "Untrust" block 
unset zone "Untrust" tcp-rst 
set zone "DMZ" tcp-rst 
set zone "VLAN" block 
unset zone "VLAN" tcp-rst 
set zone "Untrust" screen syn-flood
set zone "Untrust" screen ping-death
set zone "Untrust" screen ip-filter-src
set zone "Untrust" screen land
set zone "V1-Untrust" screen tear-drop
set zone "V1-Untrust" screen syn-flood
set zone "V1-Untrust" screen ping-death
set zone "V1-Untrust" screen ip-filter-src
set zone "V-Untrust" screen land
set interface "ethernet0/0" zone "Untrust"
set interface "ethernet0/1" zone "DMZ"
set interface "bgroup0" zone "Trust"
set interface "loopback.1" zone "Trust"
set interface bgroup0 port ethernet0/2
set interface bgroup0 port ethernet0/3
set interface bgroup0 port ethernet0/4
set interface bgroup0 port ethernet0/5
set interface bgroup0 port ethernet0/6
unset interface vlan1 ip
set interface ethernet0/0 ip 11.11.11.11/24
set interface ethernet0/0 nat
set interface bgroup0 ip 192.168.1.1/24
set interface bgroup0 nat
set interface loopback.1 ip 10.1.1.1/32
set interface loopback.1 nat
unset interface vlan1 bypass-others-ipsec
unset interface vlan1 bypass-non-ip
set interface ethernet0/0 ip manageable
set interface bgroup0 ip manageable
set interface loopback.1 ip manageable
set interface ethernet0/0 manage ping
set interface ethernet0/0 manage ssh
set interface ethernet0/0 manage snmp
set interface ethernet0/0 manage ssl
set interface ethernet0/0 manage web
set interface bgroup0 dhcp server service
set interface bgroup0 dhcp server auto
set interface bgroup0 dhcp server option gateway 192.168.1.1 
set interface bgroup0 dhcp server option netmask 255.255.255.0 
set interface bgroup0 dhcp server ip 192.168.1.33 to 192.168.1.126 
unset interface bgroup0 dhcp server config next-server-ip
set interface "serial0/0" modem settings "USR" init "AT&F"
set interface "serial0/0" modem settings "USR" active
set interface "erial0/0" modem speed 115200
set interface "serial0/0" modem retry 3
set interface "serial0/0" modem interval 10
set interface "serial0/0" modem idle-time 10
set flow tcp-mss
unset flow no-tcp-seq-check
set flow tcp-syn-check
unset flow tcp-syn-bit-check
set flow reverse-route clear-text prefer
set flow reverse-route tunnel always
set hostname SSG_FW1
set pki authority default scep mode "auto"
set pki x509 default cert-path partial
set ike respond-bad-spi 1
unset ike ikeid-enumeration
uset ike dos-protection
unset ipsec access-session enable
set ipsec access-session maximum 5000
set ipsec access-session upper-threshold 0
set ipsec access-session lower-threshold 0
set ipsec access-session dead-p2-sa-timeout 0
unset ipsec access-session log-error
unset ipsec access-session info-exch-connected
unset ipsec access-session use-error-log
set vrouter "untrust-vr"
exit
set vrouter "trust-vr"
exit
set url protocol websense
exit
set policy id 1 from "Trust" to "Untrust"  "Any" "Any" "ANY" permit 
set policy id 1
exit
set nsmgmt bulkcli reboot-timeout 60
set ssh version v2
set config lock timeout 5
unset license-key auto-update
set snmp port listen 161
set snmp port trap 162
set vrouter "untrust-vr"
exit
set vrouter "trust-vr"
unset add-default-route
exit
set vrouter "untrust-vr"