Error Details









Current switch configuration

 services {

 ssh {

 root-login allow;

 client-alive-count-max 5;

 client-alive-interval 20;

 }

 telnet {

 connection-limit 5;

 rate-limit 150;

 }

 netconf {

 ssh;

 rfc-compliant;

 yang-compliant;

 }

 web-management {

 http {

 interface irb.10;

 }

 }

 }

 auto-snapshot;

 time-zone Asia/Kolkata;

 syslog {

 file interactive-commands {

 interactive-commands any;

 }

 file messages {

 any notice;

 authorization info;

 }

 }

 processes {

 dhcp-service {

 traceoptions {

 file dhcp\_logfile size 10m;

 level all;

 flag packet;

 }

 }

 }

}

chassis {

 redundancy {

 graceful-switchover;

 }

}

interfaces {

 ge-0/0/0 {

 unit 0 {

 family ethernet-switching {

 vlan {

 members 222;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/1 {

 description Venus;

 unit 0 {

 family ethernet-switching {

 vlan {

 members 222;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/2 {

 description Mercury;

 unit 0 {

 family ethernet-switching {

 vlan {

 members 222;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/3 {

 description Chandan-Nagar;

 unit 0 {

 family ethernet-switching {

 vlan {

 members 222;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/4 {

 description Siddharth-chwal;

 unit 0 {

 family ethernet-switching {

 vlan {

 members 222;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/5 {

 description "Rajesh Dubey";

 unit 0 {

 family ethernet-switching {

 vlan {

 members 222;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/6 {

 description Shekhar-Anna;

 unit 0 {

 family ethernet-switching {

 vlan {

 members 222;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/7 {

 description Mumbai-Bank;

 unit 0 {

 family ethernet-switching {

 vlan {

 members 222;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/8 {

 unit 0 {

 family ethernet-switching {

 vlan {

 members 222;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/9 {

 unit 0 {

 family ethernet-switching {

 vlan {

 members 222;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/10 {

 unit 0 {

 family ethernet-switching {

 vlan {

 members 222;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/11 {

 unit 0 {

 family ethernet-switching {

 vlan {

 members 222;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/12 {

 unit 0 {

 family ethernet-switching {

 interface-mode access;

 vlan {

 members 222;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/13 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 ge-0/0/14 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 ge-0/0/15 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 ge-0/0/16 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 ge-0/0/17 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 ge-0/0/18 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 ge-0/0/19 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 ge-0/0/20 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 ge-0/0/21 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 ge-0/0/22 {

 unit 0 {

 family ethernet-switching {

 interface-mode access;

 vlan {

 members default;

 }

 storm-control default;

 }

 }

 }

 ge-0/0/23 {

 unit 0 {

 family ethernet-switching {

 vlan {

 members IT;

 }

 storm-control default;

 }

 }

 }

 ge-0/1/0 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 xe-0/1/0 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 ge-0/1/1 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 xe-0/1/1 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 ge-0/1/2 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 xe-0/1/2 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 ge-0/1/3 {

 description Input;

 unit 0 {

 family ethernet-switching {

 interface-mode trunk;

 vlan {

 members 222-223;

 }

 storm-control default;

 }

 }

 }

 xe-0/1/3 {

 unit 0 {

 family ethernet-switching {

 storm-control default;

 }

 }

 }

 irb {

 unit 0 {

 family inet {

 dhcp {

 vendor-id Juniper:ex2300-24t:JZ0217250019;

 }

 }

 family inet6 {

 dhcpv6-client {

 client-type stateful;

 client-ia-type ia-na;

 client-identifier duid-type duid-ll;

 vendor-id Juniper:ex2300-24t:JZ0217250019;

 }

 }

 }

 unit 10 {

 family inet {

 address 10.0.0.2/8;

 }

 }

 }

 vme {

 unit 0 {

 family inet {

 dhcp {

 vendor-id Juniper:ex2300-24t:JZ0217250019;

 }

 }

 family inet6 {

 dhcpv6-client {

 client-type stateful;

 client-ia-type ia-na;

 client-identifier duid-type duid-ll;

 vendor-id Juniper:ex2300-24t:JZ0217250019;

 }

 }

 }

 }

}

forwarding-options {

 storm-control-profiles default {

 all {

 no-broadcast;

 no-unknown-unicast;

 no-multicast;

 }

 }

}

protocols {

 router-advertisement {

 interface vme.0;

 interface irb.0;

 }

 lldp {

 interface all;

 }

 lldp-med {

 interface all;

 }

 igmp-snooping {

 vlan default;

 }

 rstp {

 interface ge-0/0/0;

 interface ge-0/0/1;

 interface ge-0/0/2;

 interface ge-0/0/3;

 interface ge-0/0/4;

 interface ge-0/0/5;

 interface ge-0/0/6;

 interface ge-0/0/7;

 interface ge-0/0/8;

 interface ge-0/0/9;

 interface ge-0/0/10;

 interface ge-0/0/11;

 interface ge-0/0/12;

 interface ge-0/0/13;

 interface ge-0/0/14;

 interface ge-0/0/15;

 interface ge-0/0/16;

 interface ge-0/0/17;

 interface ge-0/0/18;

 interface ge-0/0/19;

 interface ge-0/0/20;

 interface ge-0/0/21;

 interface ge-0/0/22;

 interface ge-0/0/23;

 interface ge-0/1/0;

 interface xe-0/1/0;

 interface ge-0/1/1;

 interface xe-0/1/1;

 interface ge-0/1/2;

 interface xe-0/1/2;

 interface ge-0/1/3;

 interface xe-0/1/3;

 }

 loop-detect;

}

vlans {

 IT {

 description "Management ID";

 vlan-id 10;

 l3-interface irb.10;

 }

 Vikhroli-Office {

 vlan-id 222;

 }

 WNET-Office {

 vlan-id 223;

 }

 default {

 vlan-id 1;

 l3-interface irb.0;

 }

}